בשני החלקים הפרוטוקול הוא ipv4

**Part A**

**Part B**

**RUDP Code Explanation**

**Part C**

**TCP: reno & Cubic**

**From Reno to Reno**

* **0% packet loss**
* **2% packet loss**
* **5% packet loss**
* **10% packet loss**

**From Reno to Cubic**

* **0% packet loss**
* **2% packet loss**
* **5% packet loss**
* **10% packet loss**

**From Cubic to Reno**

* **0% packet loss**
* **2% packet loss**
* **5% packet loss**
* **10% packet loss**

**From Cubic to Cubic**

* **0% packet loss**
* **2% packet loss**
* **5% packet loss**
* **10% packet loss**

**Part C**

**Part D - Open**